Start
Warranty and Support
What’s Included
System Requirements
Safety Instructions
Connecting
Operation
Troubleshooting
|  | # Warranty and Support ## ## Support If you experience difficulties when installing or connecting the product, please get in touch with our technical support team. A support form is available on our website: www.speedlink.com. Alternatively you can e-mail our technical support team directly: support@speedlink.com ## Limitation of liability Jöllenbeck GmbH will not be liable for damages such as damages to or loss of property, profit or turnover losses, costs for spare parts, expenses for inconveniences arising from the interruption of a service or any other damages. Claims which exceed the purchasing price of the product may not be asserted under any circumstances. ## Warranty This product is supplied with a limited warranty of two (2) years. If this product exhibits a defect within the warranty period then Jöllenbeck GmbH may repair or replace the fault product at its own discretion. To make a claim against the warranty take the defective product, together with the receipt of purchase, to the supplier you purchased the product from. ## Correct disposal This product must not be disposed of together with household waste. You are obliged to hand in used electrical equipment to an official collection point for electrical equipment. Jöllenbeck GmbH is committed to protecting as many resources as possible and with it the environment and your health as well. Help us to do this by disposing of this product at your nearest authorised collection point. You can find out where your nearest collection point is by contacting your local authority, the local disposal company or the supplier/business where you purchased this product from. ## Maintenance and repair Any repairs and maintenance work must only be performed by qualified specialists. Do not attempt to carry out repairs yourself and do not make changes to the product. ## Moisture Keep the product away from sources of moisture (rain), water and other liquids. ## Operating conditions Use the product between 5 to 40°C and with a relative humidity of 5 to 80% (non-condensing). ## Copyright © 2009 Jöllenbeck GmbH. All rights reserved. This publication may not be copied, reproduced, made retrievable or saved, neither fully or in part, nor may it be transferred or made accessible electronically, mechanically, as a photocopy, as a recording or by any other means without the express written approval of Jöllenbeck GmbH. ##  |  |  |