
Steps firmware update SL-680011-BK RETICOS RGB Gaming Mouse
--------------------------------------------------------------------------------------------------
1. Connect the mouse to a USB port on your PC.
2. Double-click "Update Tool.exe".
3. Wait until the process is finished and "PASS" appears in the window.
4. Close "Update Tool.exe" by pressing ALT+F4 on your keyboard.
5. Unplug and replug the mouse.

! In case that there is no progress in step 3 and "PASS" doesn't appear, your mouse is likely already patched.


Schritte Firmware-Update SL-680011-BK RETICOS RGB Gaming Mouse
--------------------------------------------------------------------------------------------------
1. Verbinde die Maus mit einem USB-Port deines PCs. 
2. Öffne die Datei "Update tool.exe" per Doppelklick. 
3. Warte, bis der Update-Prozess fertiggestellt ist und das Wort "PASS" im Fenster erscheint. 
4. Schließe "Update Tool.exe", indem du ALT+F4 auf deiner Tastatur drückst. 
5. Trenne die Maus vom PC und schließe sie dann erneut an. 

! Falls in Schritt 3 kein Fortschritt erkennbar ist und "PASS" nicht erscheint, ist deine Maus möglicherweise bereits aktualisiert. 